

**Infinite Uptime IDE+ Calibration Procedure**

1/ Make sure that the IDE+ has been flashed with the latest version of the firmware “Butterfly Firmware”.

2/